2020-7-7

1、Solve the scan issue

2、Solve the scramble issue

1、If your radio version starts from BQXXX, please press PTT + P1 at the same time to power on and indicator will light green.

2、open the updating software and set Baud rate as 57600 and choose the correct comm port

open the firmware and press updata

3、please kindly note that during updating, if updating is interrupted, please do not turn on the radio, otherwise, the chip will be broken and radio won't work forever, then it will need to change chip, please keep radio in updating mode and turn off the updating software and open it again and press reset in the updating software, after finish the reset, just update again

latest firmware is UV88\_Eng\_BQ1\_30\_20200629

