
Before updating, please check your original firmware version, it should start with letter of BS



2022-12-20

A\_SWS181\_Uv88\_Eng\_BSV1\_60\_20221220

To solve the issue that when you release second side key and exit monitor mode, radio still can hear the signals, but indicator is off

2022-1-5

Solve the issue that in FM radio mode, when you press MON, the radio enter into monitor mode, but when signal disappears, FM radio didn't recover

please kindly note that following serial number use the new MCU, while updating software and operation and firmware are all different, and on the radio aluminum chassis, it will have one label saying NEW

EU version: 2111A00031-2111A00530

US version: Serial number starts from 2105A00694



1、please press PTT to power on and display will flash

2、open the updating software and set Baud rate as 57600 and choose the correct com port

open the firmware and press update

